{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":62,"n_cols":11,"rows_kept":62,"merged":[[0,0,0,10],[2,0,9,0],[10,0,17,0],[18,0,29,0],[30,0,35,0],[36,0,46,0],[47,0,49,0],[50,0,59,0],[60,0,60,1],[60,2,60,10],[61,0,61,10]],"flags":["formulas_cached_only"]}
["天心经开区暮云片区六条路及芙蓉西侧绿化景观提质改造工程检测清单"]
["检测部位","检测项目","检测内容","单位","预估工程量","收费标准单价","优惠后单价","折扣优惠率","优惠后小计","收费依据","备注"]
["土路基","土工","击实、筛分、液塑限、CBR","组"]
[null,"路基压实度","压实度","点"]
[null,"回弹模量","回弹模量","点"]
[null,"片石","立方体抗压","组"]
[null,"沙砾石","密度、级配、压碎值、吸水率、粘附性等","组"]
[null,"土工格栅","拉伸、撕破、穿透","组"]
[null,"弯沉","弯沉","点"]
[null,"承载力试验","触探","点"]
["水稳层","水稳配合比设计","配合比","组"]
[null,"级配碎石配合比设计","配合比","组"]
[null,"基层卵碎石原材检测","密度、级配、压碎值、吸水率、粘附性等","组"]
[null,"水稳压实度","压实度","点"]
[null,"水泥剂量","水泥掺量","组"]
[null,"水稳基层钻芯","厚度","点"]
[null,"无侧限抗压强度","强度","组"]
[null,"弯沉","弯沉","点"]
["沥青层","沥青配合比设计","配合比","组"]
[null,"沥青混合料","油石比、级配、马歇尔","组"]
[null,"粗集料（原材料）","密度、级配、压碎值、吸水率、粘附性等","组"]
[null,"细集料（原材料）","密度、砂当量、级配、含泥量等常规","组"]
[null,"矿粉（原材料）","密度、级配、含水率等常规","组"]
[null,"沥青三大指标","延度、软化点、针入度等常规","组"]
[null,"乳化沥青","常规","组"]
[null,"平整度测试","平整度","km车道"]
[null,"钻芯压实度","压实度","点"]
[null,"沥青面层厚度","厚度","点"]
[null,"弯沉","弯沉","点"]
[null,"混凝土配合比设计","配合比","组"]
["排水工程","HDPE大类管材","规格、拉伸、伸长率、断裂、烘箱、冲击","组"]
[null,"钢筋混凝土排水管","外观、尺寸、外压等常规","组"]
[null,"管道沟槽基坑触探","触探","点"]
[null,"闭水试验","闭水试验","段"]
[null,"PPR给水管","规格、拉伸、伸长率、断裂、烘箱、冲击","组"]
[null,"管道回填压实度","压实度","点"]
["交通工程","立柱竖直度","常规","组"]
[null,"标志基础尺寸","常规","组"]
[null,"标志金属构件镀层厚度","常规","组"]
[null,"标线线段长度","常规","组"]
[null,"标线宽度","常规","组"]
[null,"标线横向偏位","常规","组"]
[null,"标线纵向间距","常规","组"]
[null,"标线逆反射系数","常规","组"]
[null,"抗滑值","常规","组"]
[null,"试块抗压","常规","组"]
[null,"地脚螺栓","常规","组"]
["照明工程","电线电缆","印刷标志、外径测量、绝缘厚度、导体电","组"]
[null,"大类管材","规格、拉伸、伸长率、断裂、烘箱、冲击","组"]
[null,"接地电阻","接地电阻","点"]
["材料","水泥","强度、安定、凝结、细度","组"]
[null,"砂","密度、砂当量、级配、含泥量等常规","组"]
[null,"沙砾、卵石","密度、级配、压碎值、吸水率、粘附性等","组"]
[null,"路面砖","常规","组"]
[null,"钢筋原材","抗拉、冷弯、质量偏差","组"]
[null,"砼配合比设计","配合比","组"]
[null,"砂浆配合比设计","配合比","组"]
[null,"砼试块抗折","常规","组"]
[null,"砼试块抗压","强度","组"]
[null,"砂浆试块抗压","强度","组"]
["优惠后合计："]
[" 备注：部分检测工程量为预估工程量，最终结算以实际发生为准。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}